**Class A and B Subnetting Practice**

Network Address: 178.26.0.0 (Class B) Subnet Sizes: 9500, 12000, 800, 3500, 35 and 2 WAN Links

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Subnet Size** | **Increment/Octet** | **Network Address** | **Broadcast Address** | **Subnet Mask** |
|  |  | 178.26.0.0 |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Network Address: 104.0.0.0 (Class A) Subnet Sizes: 450000, 49000, 95000, 2200, 95, 100, 25 and 1 WAN Links

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Subnet Size** | **Increment/Octet** | **Network Address** | **Broadcast Address** | **Subnet Mask** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |